# MARKING OF THE PRODUCT

# 09.04.2025

# PRODUCTS COVERED BY THE CERTIFICATE

Every product must be provided with a fixed and easily legible label or marking containing at least the following information:

• certificate number;

• normative document on the basis of which the certificate was issued and to which the product complies;

• performance covered by the certificate (fire resistance and/or smoke control and/or self-closing class)\*;

• name of the manufacturer (address may also be included);

• type and/or name of the product;

• serial number or unique reference number of the product;

• year of manufacture (if the serial number or unique reference number of the product does not include a reference to the year);

• the certification mark of Kiwa Estonia OÜ or the inscription “Kiwa certified” shall be placed at the top of the label.

• In the case of a CPR certificate, the “CE” symbol and the identification number of the product certification body may be added to the label.

**\*The manufacturer may declare performance only for the complete end product.**

Label dimensions (W x H, mm): 25-40 x 55-70.

The label must be located on the frame and edge of the leaf of the opening opening, on the frame of the non-opening opening.

*Additional obligations in the harmonized field:*

*When marketing its product, the manufacturer shall draw up a declaration of performance of the product in accordance with Regulation (EU) No 305/2011 of the European Parliament and of the Council.*

*The CE marking, drawn up in accordance with Regulation (EU) No 305/2011 of the European Parliament and of the Council, shall be provided with the product sales documentation.*

**Näidised:**

|  |
| --- |
| **A blue and white sign with text  AI-generated content may be incorrect.**1336-CPR-0001**EN 14351-1:2006 + A2:2016****AS ABC****Street x****12345 Tallinn** type P50ID No 25877-18 |
| **cid:image005.png@01D38572.5036A200****1336** |

|  |
| --- |
| **A blue and white sign with text  AI-generated content may be incorrect.**1336-CPR-xxxx**EN 16034:2014****EI230****Sa / S200****C5****AS ABC**fire doortype P50ID No xxxx-yy |

|  |
| --- |
| **A blue and white sign with text  AI-generated content may be incorrect.**ET-xxxx-yy**EN 16034:2014****EI130****Sa / S200****C5****AS ABC**fire doortype P50ID No xxxxx-xx**yyyy** |

|  |
| --- |
| **A blue and white sign with text  AI-generated content may be incorrect.**1336-CPR-xxxx**EN 16034:2014****AS ABC****Street x****12345 Tallinn** type P50ID No xxxx-yy**EI230****Sa / S200****C5** |
| **cid:image005.png@01D38572.5036A200****1336** |

|  |
| --- |
| Kiwa certifiedET-xxxx-yy**EN 16034:2014****AS ABC**fire door typeP50ID No xxxxx-yy **EI230****Sa / S200****C5** |

|  |
| --- |
| Kiwa certified1336-CPR-xxxx**EN 16034:2014****EI230****AS ABC**openable window type P50ID No xxxxx-xx**yyyy** |

|  |
| --- |
| ET-xxxx-yy**TS-ET-xxxx****EI60****AS ABC**tuletõkkeakentüüp P50ID nr xxxx-yy |

|  |
| --- |
| Kiwa certifiedET-xxxx-yy**TS-ET-xxxx****EI30****AS ABC**fire resistant wall type P50ID No xxxxx-xx**yyyy** |

|  |
| --- |
| 1336-CPR-xxxx**EN 14351-1:2006 + A2:2016****AS ABC**välisukstüüp P50ID nr xxxxx-xx**yyyy** |

|  |
| --- |
| Kiwa certified1336-CPR-0001**EN 16034:2014****AS ABC****Street x****12345 Tallinn** type P50ID No xxxx-yy **EI230** |
| **cid:image005.png@01D38572.5036A200****1336** |

# PRODUCTS COVERED BY EXPERT OPINION

Openable and non-openable fillings must be provided with a fixed and easily legible label or mark containing at least the following information:

• expert opinion number;

• performance covered by the expert opinion (fire resistance and/or smoke control class)\*;

• manufacturer's name;

• product type and/or name;

• year of manufacture;

• the expert opinion symbol of Kiwa Estonia OÜ or the inscription "Kiwa expert opinion" is placed at the top of the label.

\*The manufacturer may declare performance only for the complete end product.

Label dimensions (W x H, mm): 25-40 x 55-70.

The label must be located on the frame and leaf edge of the opening filling, and on the frame of the non-opening filling.

**Examples:**

|  |  |  |  |
| --- | --- | --- | --- |
|

|  |
| --- |
| **xxx-yy-xxxx**Toote tüüp**EI230****Sa/S200****AS ABC** yyyy |

|  |
| --- |
| Kiwa ekspertarvamus**xxx-yy-xxxx**Toote tüüp**EI230****Sa/S200****AS ABC** yyyy |

3. JOINT FILLER, PENTAGE MATERIALS, FIRE PROTECTION EQUIPMENTThe product must contain at least the following information:• certification mark with reference to the certificate number\*;• performance covered by the certificate (fire resistance class / reaction to fire class);• name and address of the manufacturer;• type and/or name of the product;• batch number and/or date of manufacture of the product.Example of the certification mark:  \* *The placement of the certification mark on the product must not be misleading* |  |